**Deimos ECO Harnesses (Climber Style)**

These harnesses are designed for rope parks that have challenge courses, zip lines rides, as well as drop towers and king swings.

|  |  |
| --- | --- |
| **ECO Sit** C:\Users\user\Desktop\eco sit2.jpg | Designed rope parks and zip lines:* Light full body harness. Very easy to walk in.
* One Size fits all!
* Waist Size (up to 52” 132 cm).
* Rider Age: 8 and up.
* No rear D-Ring.
* Certification: EN 12277
* Tested to more than 4000lbs.
* Weight: 430g.
* Size (XS-XL)

Impact ForceC:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpg |
| **ECO K-Lite** C:\Users\tc\Desktop\eco_K_LITE2.jpg | Designed rope parks and zip lines:* Light full body harness for small children. Very easy to walk in.
* Waist Size (58 to 90 cm).
* Leg Size (31-56 cm).
* Max height (145cm).
* Rider Age: 4-11.
* Has Rear D-Ring.
* Certification: UIAA105
* Tested to more than 4000lbs.
* Weight: 500g
* Size (XS-S).

Impact ForceC:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpg |

|  |  |
| --- | --- |
| **ECO Lite**C:\Users\HP user\Desktop\ECO Lite 500.jpg | Designed for rope parks and zip lines:* Light full body harness, very easy to walk in.
* Available in one size only.
* Waist Size (61 – 147 cm).
* Rider Age: 8 and up.
* Has rear D-Ring.
* Certification: UIAA105.
* Tested to breaking force of 6362 lbs.
* Tested to more than 4000lbs.
* Weight: 600g
* Size (S-XL)

Impact ForceC:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpg |
| **ECO Lite III**C:\Users\user\Desktop\ECO Lite III 500.jpg | Designed for rope parks and zip lines:* Light full body harness, very easy to walk in.
* Available in one size only (S-XXL).
* Waist Size (61 cm to 147 cm).
* Rider Age: 8 and up.
* Has rear a D-Ring.
* Certification: EN 813 358 361

(feet first and heads first tested).* Tested to more than 4000lbs.
* Weight: 600g
* Size (S-XL)

Impact ForceC:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpg |

|  |  |
| --- | --- |
| **ECO 5000**C:\Users\user\Desktop\ECO_5000_FRNT.jpg | **Designed for both rope parks and zip lines.*** Medium weight, full body harness for use in adventure parks. Fully padded shoulder straps.
* Available in one size only (S-XXL)
* Waist Size (61 cm to 147 cm).
* Rider Age: 8 and up.
* Has no rear D-Ring or leg padding.
* Certification: EN 12277
* Feet first and heads first tested.
* Tested to more than 5000lbs.
* Weight: 800g
* Size (S-XL)

Max Impact ForceC:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpg |
| **ECO D-Lite (S) and (L)****(rear view)**C:\Users\tc\Desktop\eco_dlight_rear_SM.jpg | **Designed for both rope parks and zip lines.*** Medium weight, full body harness for use in adventure parks. Fully padded legs and waist straps.
* Two large gear Loops
* Certifications: CE 1019 , EN 12277
* Tested to more than 4000lbs.
* Weight: 850g and 900g

Available in two sizes:* S (83 – 135 cm) Small Waist Padding
* L (94 – 145 cm) Large Waist Padding

Max Impact ForceC:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpg |

|  |  |
| --- | --- |
| **ECO Pro**C:\Users\tc\Desktop\ECO_Pro_Jas.jpg | Designed for Leap Towers and Ziplines:* A fully padded full body harness designed especially for Leap Towers. No quick release buckles.
* Available in two sizes
* Three tie in points
* Two large gear loops
* Includes 50kN locking carabiner
* Certifications: EN361, 358, 813
* Tested to more than 4000lbs.
* Weight: 2223g >4000 lbs
* Size (XS-M) – (58 – 111cm)
* Size M-XL – (78 – 142cm)

Max Impact ForceC:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpg |
| **FreeStyle GM**C:\Users\user\Desktop\Deimos Images\FreeStyle_GM_500.jpg | **Function:** climb and zip.Easy to walk in – the best option for course with lots of walking and long zip lines.One harness for both rope parks and dual zip lines.Works with all trolley types.**Available in three sizes :**XS-M Waist 22” to 44”M-XL Waist 27” to 51”L - XXL Waist 27” to 54”**Function:** Full chair zip or climbing harness.Weight – around 1.5 kgCertified EN 1651Front loop tested to more than 5800 lbs!Max Impact ForceC:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpg |

|  |  |
| --- | --- |
| **WallTee**WallTee Harness.jpg | **Function:** Zip Lines only.Highest comfort – has padded wooden seat.Spreader bar required.**Available in three sizes :**(XS-M) Rider’s age 2-11.(S-L) Rider’s age 8 and up.(L- XXL) For Rider’s 220 to 300 lbs!**Function:** ZipLine Chair.Weight – around 2.5 kgSize S-L - Certified EN 1651Others sizes have not been tested yet.Tested to more than 4000 lbs!Max Impact ForceC:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpg |

|  |
| --- |
| **Impact Force Indicator**This is a general indication of how comfortable the harness will feel if you take a fall. Typically all harnesses are tested and certified to at least 4000 lbs.C:\Users\tc\Desktop\Deimos Images\500lbs.jpg Not comfortable if you fall (for high walk ways).C:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpg Has extra webbing in seat for comfort (for ziplines).C:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpg has padded legs and waist (for challenge courses and ziplines).C:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpg Designed for big falls (for tower leaps and ziplines). |