**Deimos ECO Harnesses (Climber Style)**

These harnesses are designed for rope parks that have challenge courses, zip lines rides, as well as drop towers and king swings.

|  |  |
| --- | --- |
| **ECO Sit**  C:\Users\user\Desktop\eco sit2.jpg | Designed rope parks and zip lines:  * Light full body harness. Very easy to walk in. * One Size fits all! * Waist Size (up to 52” 132 cm). * Rider Age: 8 and up. * No rear D-Ring. * Certification: EN 12277 * Tested to more than 4000lbs. * Weight: 430g. * Size (XS-XL)   Impact Force  C:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpg |
| **ECO K-Lite**  C:\Users\tc\Desktop\eco_K_LITE2.jpg | Designed rope parks and zip lines:  * Light full body harness for small children. Very easy to walk in. * Waist Size (58 to 90 cm). * Leg Size (31-56 cm). * Max height (145cm). * Rider Age: 4-11. * Has Rear D-Ring. * Certification: UIAA105 * Tested to more than 4000lbs. * Weight: 500g * Size (XS-S).   Impact Force  C:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpg |

|  |  |
| --- | --- |
| **ECO Lite**  C:\Users\HP user\Desktop\ECO Lite 500.jpg | Designed for rope parks and zip lines:  * Light full body harness, very easy to walk in. * Available in one size only. * Waist Size (61 – 147 cm). * Rider Age: 8 and up. * Has rear D-Ring. * Certification: UIAA105. * Tested to breaking force of 6362 lbs. * Tested to more than 4000lbs. * Weight: 600g * Size (S-XL)   Impact Force  C:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpg |
| **ECO Lite III**  C:\Users\user\Desktop\ECO Lite III 500.jpg | Designed for rope parks and zip lines:  * Light full body harness, very easy to walk in. * Available in one size only (S-XXL). * Waist Size (61 cm to 147 cm). * Rider Age: 8 and up. * Has rear a D-Ring. * Certification: EN 813 358 361   (feet first and heads first tested).   * Tested to more than 4000lbs. * Weight: 600g * Size (S-XL)   Impact Force  C:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpg |

|  |  |
| --- | --- |
| **ECO 5000**  C:\Users\user\Desktop\ECO_5000_FRNT.jpg | **Designed for both rope parks and zip lines.**   * Medium weight, full body harness for use in adventure parks. Fully padded shoulder straps. * Available in one size only (S-XXL) * Waist Size (61 cm to 147 cm). * Rider Age: 8 and up. * Has no rear D-Ring or leg padding. * Certification: EN 12277 * Feet first and heads first tested. * Tested to more than 5000lbs. * Weight: 800g * Size (S-XL)   Max Impact Force  C:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpg |
| **ECO D-Lite (S) and (L)**  **(rear view)**  C:\Users\tc\Desktop\eco_dlight_rear_SM.jpg | **Designed for both rope parks and zip lines.**   * Medium weight, full body harness for use in adventure parks. Fully padded legs and waist straps. * Two large gear Loops * Certifications: CE 1019 , EN 12277 * Tested to more than 4000lbs. * Weight: 850g and 900g   Available in two sizes:   * S (83 – 135 cm) Small Waist Padding * L (94 – 145 cm) Large Waist Padding   Max Impact Force  C:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpg |

|  |  |  |  |
| --- | --- | --- | --- |
| **ECO Pro**  C:\Users\tc\Desktop\ECO_Pro_Jas.jpg | Designed for Leap Towers and Ziplines:  * A fully padded full body harness designed especially for Leap Towers. No quick release buckles. * Available in two sizes * Three tie in points * Two large gear loops * Includes 50kN locking carabiner * Certifications: EN361, 358, 813 * Tested to more than 4000lbs. * Weight: 2223g >4000 lbs * Size (XS-M) – (58 – 111cm) * Size M-XL – (78 – 142cm)   Max Impact Force  C:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpg | | |
| **FreeStyle GM**  C:\Users\user\Desktop\Deimos Images\FreeStyle_GM_500.jpg | | **Function:** climb and zip.  Easy to walk in – the best option for course with lots of walking and long zip lines.  One harness for both rope parks and dual zip lines.  Works with all trolley types.  **Available in three sizes :**  XS-M Waist 22” to 44”  M-XL Waist 27” to 51”  L - XXL Waist 27” to 54”  **Function:** Full chair zip or climbing harness.  Weight – around 1.5 kg  Certified EN 1651  Front loop tested to more than 5800 lbs!  Max Impact Force  C:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpg |

|  |  |
| --- | --- |
| **WallTee**  WallTee Harness.jpg | **Function:** Zip Lines only.  Highest comfort – has padded wooden seat.  Spreader bar required.  **Available in three sizes :**  (XS-M) Rider’s age 2-11.  (S-L) Rider’s age 8 and up.  (L- XXL) For Rider’s 220 to 300 lbs!  **Function:** ZipLine Chair.  Weight – around 2.5 kg  Size S-L - Certified EN 1651  Others sizes have not been tested yet.  Tested to more than 4000 lbs!  Max Impact Force  C:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpg |

|  |
| --- |
| **Impact Force Indicator**  This is a general indication of how comfortable the harness will feel if you take a fall. Typically all harnesses are tested and certified to at least 4000 lbs.  C:\Users\tc\Desktop\Deimos Images\500lbs.jpg Not comfortable if you fall (for high walk ways).  C:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpg Has extra webbing in seat for comfort (for ziplines).  C:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpg has padded legs and waist (for challenge courses and ziplines).  C:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpgC:\Users\tc\Desktop\Deimos Images\500lbs.jpg Designed for big falls (for tower leaps and ziplines). |